(module usb30 (layer F.Cu) (tedit 5D4941FD)
  (clearance 0.127)
  (fp_text reference REF** (at 0 3.29) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value usb30 (at 0 -3.28) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_arc (start 2.88 0) (end 2.88 1.28) (angle -180) (layer F.SilkS) (width 0.15))
  (fp_arc (start -2.88 0) (end -2.88 -1.28) (angle -180) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.88 -1.28) (end -2.88 -1.28) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.83 1.28) (end 2.88 1.28) (layer F.SilkS) (width 0.15))
  (pad A1 thru_hole circle (at -3.15 -0.7) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask))
  (pad S1 thru_hole roundrect (at 2 -1.93) (size 2.3 0.9) (drill oval 1.9 0.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
  (pad S1 thru_hole roundrect (at -2 -1.93) (size 2.3 0.9) (drill oval 1.9 0.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
  (pad S1 thru_hole roundrect (at -2 1.93) (size 2.3 0.9) (drill oval 1.9 0.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
  (pad S1 thru_hole roundrect (at 2 1.93) (size 2.3 0.9) (drill oval 1.9 0.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
  (pad A4 thru_hole circle (at -2.25 -0.7) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask))
  (pad A5 thru_hole circle (at -1.35 -0.7) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask))
  (pad A6 thru_hole circle (at -0.45 -0.7) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask))
  (pad A7 thru_hole circle (at 0.45 -0.7) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask))
  (pad A9 thru_hole circle (at 2.25 -0.7) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask))
  (pad A12 thru_hole circle (at 3.15 -0.7) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask))
  (pad B1 thru_hole circle (at 3.15 0.7) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask))
  (pad B4 thru_hole circle (at 2.25 0.7) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask))
  (pad B5 thru_hole circle (at 1.35 0.7) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask))
  (pad B6 thru_hole circle (at 0.45 0.7) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask))
  (pad B7 thru_hole circle (at -0.45 0.7) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask))
  (pad B9 thru_hole circle (at -2.25 0.7) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask))
  (pad B12 thru_hole circle (at -3.15 0.7) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask))
)
